/\*

u8g\_com\_arduino\_uc\_i2c.c

com interface for arduino (AND atmega) and the SSDxxxx chip (SOLOMON) variant

I2C protocol

ToDo: Rename this to u8g\_com\_avr\_ssd\_i2c.c

Universal 8bit Graphics Library

Copyright (c) 2012, olikraus@gmail.com

All rights reserved.

Redistribution and use in source and binary forms, with or without modification,

are permitted provided that the following conditions are met:

\* Redistributions of source code must retain the above copyright notice, this list

of conditions and the following disclaimer.

\* Redistributions in binary form must reproduce the above copyright notice, this

list of conditions and the following disclaimer in the documentation and/or other

materials provided with the distribution.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND

CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES,

INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF

MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE

DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR

CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,

SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT

NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;

LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER

CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT,

STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)

ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF

ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Special pin usage:

U8G\_PI\_I2C\_OPTION additional options

U8G\_PI\_A0\_STATE used to store the last value of the command/data register selection

U8G\_PI\_SET\_A0 1: Signal request to update I2C device with new A0\_STATE, 0: Do nothing, A0\_STATE matches I2C device

U8G\_PI\_SCL clock line (NOT USED)

U8G\_PI\_SDA data line (NOT USED)

U8G\_PI\_RESET reset line (currently disabled, see below)

Protocol:

SLA, Cmd/Data Selection, Arguments

The command/data register is selected by a special instruction byte, which is sent after SLA

The continue bit is always 0 so that a (re)start is equired for the change from cmd to/data mode

\*/

#include "u8g.h"

#if defined(U8G\_WITH\_PINLIST)

#define DOGM240\_SLA\_CMD (0x38\*2)

#define DOGM240\_SLA\_DATA (0x39\*2)

uint8\_t u8g\_com\_arduino\_uc\_start\_sequence(u8g\_t \*u8g)

{

/\* are we requested to set the a0 state? \*/

if ( u8g->pin\_list[U8G\_PI\_SET\_A0] == 0 )

return 1;

if ( u8g->pin\_list[U8G\_PI\_A0\_STATE] == 0 )

{

if ( u8g\_i2c\_start(DOGM240\_SLA\_CMD) == 0 )

return 0;

}

else

{

if ( u8g\_i2c\_start(DOGM240\_SLA\_DATA) == 0 )

return 0;

}

u8g->pin\_list[U8G\_PI\_SET\_A0] = 0;

return 1;

}

uint8\_t u8g\_com\_arduino\_uc\_i2c\_fn(u8g\_t \*u8g, uint8\_t msg, uint8\_t arg\_val, void \*arg\_ptr)

{

switch(msg)

{

case U8G\_COM\_MSG\_INIT:

//u8g\_com\_arduino\_digital\_write(u8g, U8G\_PI\_SCL, HIGH);

//u8g\_com\_arduino\_digital\_write(u8g, U8G\_PI\_SDA, HIGH);

//u8g->pin\_list[U8G\_PI\_A0\_STATE] = 0; /\* inital RS state: unknown mode \*/

u8g\_i2c\_init(u8g->pin\_list[U8G\_PI\_I2C\_OPTION]);

break;

case U8G\_COM\_MSG\_STOP:

break;

case U8G\_COM\_MSG\_RESET:

/\* Currently disabled, but it could be enable. Previous restrictions have been removed \*/

/\* u8g\_com\_arduino\_digital\_write(u8g, U8G\_PI\_RESET, arg\_val); \*/

break;

case U8G\_COM\_MSG\_CHIP\_SELECT:

u8g->pin\_list[U8G\_PI\_A0\_STATE] = 0;

u8g->pin\_list[U8G\_PI\_SET\_A0] = 1; /\* force a0 to set again, also forces start condition \*/

if ( arg\_val == 0 )

{

/\* disable chip, send stop condition \*/

u8g\_i2c\_stop();

}

else

{

/\* enable, do nothing: any byte writing will trigger the i2c start \*/

}

break;

case U8G\_COM\_MSG\_WRITE\_BYTE:

//u8g->pin\_list[U8G\_PI\_SET\_A0] = 1;

if ( u8g\_com\_arduino\_uc\_start\_sequence(u8g) == 0 )

return u8g\_i2c\_stop(), 0;

if ( u8g\_i2c\_send\_byte(arg\_val) == 0 )

return u8g\_i2c\_stop(), 0;

// u8g\_i2c\_stop();

break;

case U8G\_COM\_MSG\_WRITE\_SEQ:

//u8g->pin\_list[U8G\_PI\_SET\_A0] = 1;

if ( u8g\_com\_arduino\_uc\_start\_sequence(u8g) == 0 )

return u8g\_i2c\_stop(), 0;

{

register uint8\_t \*ptr = arg\_ptr;

while( arg\_val > 0 )

{

if ( u8g\_i2c\_send\_byte(\*ptr++) == 0 )

return u8g\_i2c\_stop(), 0;

arg\_val--;

}

}

// u8g\_i2c\_stop();

break;

case U8G\_COM\_MSG\_WRITE\_SEQ\_P:

//u8g->pin\_list[U8G\_PI\_SET\_A0] = 1;

if ( u8g\_com\_arduino\_uc\_start\_sequence(u8g) == 0 )

return u8g\_i2c\_stop(), 0;

{

register uint8\_t \*ptr = arg\_ptr;

while( arg\_val > 0 )

{

if ( u8g\_i2c\_send\_byte(u8g\_pgm\_read(ptr)) == 0 )

return 0;

ptr++;

arg\_val--;

}

}

// u8g\_i2c\_stop();

break;

case U8G\_COM\_MSG\_ADDRESS: /\* define cmd (arg\_val = 0) or data mode (arg\_val = 1) \*/

u8g->pin\_list[U8G\_PI\_A0\_STATE] = arg\_val;

u8g->pin\_list[U8G\_PI\_SET\_A0] = 1; /\* force a0 to set again \*/

#ifdef OLD\_CODE

if ( i2c\_state != 0 )

{

u8g\_i2c\_stop();

i2c\_state = 0;

}

if ( u8g\_com\_arduino\_uc\_start\_sequence(arg\_val) == 0 )

return 0;

/\* setup bus, might be a repeated start \*/

/\*

if ( u8g\_i2c\_start(I2C\_SLA) == 0 )

return 0;

if ( arg\_val == 0 )

{

i2c\_state = 1;

if ( u8g\_i2c\_send\_byte(I2C\_CMD\_MODE) == 0 )

return 0;

}

else

{

i2c\_state = 2;

if ( u8g\_i2c\_send\_byte(I2C\_DATA\_MODE) == 0 )

return 0;

}

\*/

#endif

break;

}

return 1;

}

#else /\* defined(U8G\_WITH\_PINLIST) \*/

uint8\_t u8g\_com\_arduino\_uc\_i2c\_fn(u8g\_t \*u8g, uint8\_t msg, uint8\_t arg\_val, void \*arg\_ptr)

{

return 1;

}

#endif /\* defined(U8G\_WITH\_PINLIST) \*/